Release 14.7 - par P.20131013 (lin64)
Copyright (c) 1995-2013 Xilinx, Inc.  All rights reserved.

Wed May  3 20:03:56 2023


INFO: The IO information is provided in three file formats as part of the Place and Route (PAR) process.  These formats are:
1. The <design name>_pad.txt file (this file) designed to provide information on IO usage in a human readable ASCII text format viewable through common text editors.
2. The <design namd>_pad.csv file for use with spreadsheet programs such as MS Excel. This file can also be read by PACE to communicate post PAR IO information.
3. The <design name>.pad file designed for parsing by customers.  It uses the "|" as a data field separator.

INPUT FILE:       Minimig1_map.ncd
OUTPUT FILE:      Minimig1_pad.txt
PART TYPE:        xc3s400
SPEED GRADE:      -4
PACKAGE:          pq208

Pinout by Pin Number:

+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|Pin Number|Signal Name    |Pin Usage|Pin Name           |Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|IO Register|Signal Integrity|
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|P1        |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P2        |green<2>       |IOB      |IO_L01P_7/VRN_7    |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P3        |green<3>       |IOB      |IO_L01N_7/VRP_7    |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P4        |red<0>         |IOB      |IO_L16P_7/VREF_7   |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P5        |red<1>         |IOB      |IO_L16N_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P6        |               |         |VCCO_7             |         |           |7             |          |         |           |         |3.30   |          |           |                |
|P7        |red<2>         |IOB      |IO_L19P_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P8        |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P9        |red<3>         |IOB      |IO_L19N_7/VREF_7   |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P10       |kbddat         |IOB      |IO_L20P_7          |BIDIR    |LVCMOS33   |7             |12        |SLOW     |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P11       |kbdclk         |IOB      |IO_L20N_7          |BIDIR    |LVCMOS33   |7             |12        |SLOW     |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P12       |msdat          |IOB      |IO_L21P_7          |BIDIR    |LVCMOS33   |7             |12        |SLOW     |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P13       |msclk          |IOB      |IO_L21N_7          |BIDIR    |LVCMOS33   |7             |12        |SLOW     |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P14       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P15       |_ram_ce<2>     |IOB      |IO_L22P_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P16       |               |DIFFS    |IO_L22N_7          |UNUSED   |           |7             |          |         |           |         |       |          |           |                |
|P17       |               |         |VCCAUX             |         |           |              |          |         |           |         |2.5    |          |           |                |
|P18       |_ram_ce<3>     |IOB      |IO_L23P_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P19       |sdo            |IOB      |IO_L23N_7          |BIDIR    |LVCMOS33   |7             |4         |SLOW     |NONE**     |NONE     |       |LOCATED   |NO         |NONE            |
|P20       |_ram_ce<1>     |IOB      |IO_L24P_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P21       |ram_address<5> |IOB      |IO_L24N_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P22       |ram_address<4> |IOB      |IO_L39P_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P23       |               |         |VCCO_7             |         |           |7             |          |         |           |         |3.30   |          |           |                |
|P24       |ram_address<3> |IOB      |IO_L39N_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P25       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P26       |ram_address<2> |IOB      |IO_L40P_7          |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P27       |ram_address<1> |IOB      |IO_L40N_7/VREF_7   |OUTPUT   |LVCMOS33   |7             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P28       |_ram_ce<0>     |IOB      |IO_L40P_6/VREF_6   |OUTPUT   |LVCMOS33   |6             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P29       |ram_data<0>    |IOB      |IO_L40N_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P30       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P31       |ram_data<1>    |IOB      |IO_L39P_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P32       |               |         |VCCO_6             |         |           |6             |          |         |           |         |3.30   |          |           |                |
|P33       |ram_data<2>    |IOB      |IO_L39N_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P34       |ram_data<3>    |IOB      |IO_L24P_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P35       |ram_address<6> |IOB      |IO_L24N_6/VREF_6   |OUTPUT   |LVCMOS33   |6             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P36       |ram_address<7> |IOB      |IO_L23P_6          |OUTPUT   |LVCMOS33   |6             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P37       |ram_address<8> |IOB      |IO_L23N_6          |OUTPUT   |LVCMOS33   |6             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P38       |               |         |VCCAUX             |         |           |              |          |         |           |         |2.5    |          |           |                |
|P39       |_ram_oe        |IOB      |IO_L22P_6          |OUTPUT   |LVCMOS33   |6             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P40       |_ram_bhe       |IOB      |IO_L22N_6          |OUTPUT   |LVCMOS33   |6             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P41       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P42       |_ram_ble       |IOB      |IO_L21P_6          |OUTPUT   |LVCMOS33   |6             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P43       |ram_data<15>   |IOB      |IO_L21N_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P44       |ram_data<14>   |IOB      |IO_L20P_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P45       |ram_data<13>   |IOB      |IO_L20N_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P46       |ram_data<12>   |IOB      |IO_L19P_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P47       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P48       |ram_data<11>   |IOB      |IO_L19N_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P49       |               |         |VCCO_6             |         |           |6             |          |         |           |         |3.30   |          |           |                |
|P50       |ram_data<10>   |IOB      |IO/VREF_6          |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P51       |ram_data<9>    |IOB      |IO_L01P_6/VRN_6    |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P52       |ram_data<8>    |IOB      |IO_L01N_6/VRP_6    |BIDIR    |LVCMOS33   |6             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P53       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P54       |               |         |M1                 |         |           |              |          |         |           |         |       |          |           |                |
|P55       |               |         |M0                 |         |           |              |          |         |           |         |       |          |           |                |
|P56       |               |         |M2                 |         |           |              |          |         |           |         |       |          |           |                |
|P57       |ram_address<9> |IOB      |IO_L01P_5/CS_B     |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P58       |ram_address<10>|IOB      |IO_L01N_5/RDWR_B   |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P59       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P60       |               |         |VCCO_5             |         |           |5             |          |         |           |         |3.30   |          |           |                |
|P61       |ram_address<11>|IOB      |IO_L10P_5/VRN_5    |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P62       |ram_address<12>|IOB      |IO_L10N_5/VRP_5    |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P63       |ram_address<13>|IOB      |IO                 |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P64       |ram_address<14>|IOB      |IO_L27P_5          |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P65       |ram_data<4>    |IOB      |IO_L27N_5/VREF_5   |BIDIR    |LVCMOS33   |5             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P66       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P67       |ram_data<5>    |IOB      |IO_L28P_5/D7       |BIDIR    |LVCMOS33   |5             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P68       |ram_data<6>    |IOB      |IO_L28N_5/D6       |BIDIR    |LVCMOS33   |5             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P69       |               |         |VCCAUX             |         |           |              |          |         |           |         |2.5    |          |           |                |
|P70       |               |         |VCCINT             |         |           |              |          |         |           |         |1.2    |          |           |                |
|P71       |ram_data<7>    |IOB      |IO                 |BIDIR    |LVCMOS33   |5             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P72       |_ram_we        |IOB      |IO_L31P_5/D5       |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P73       |               |         |VCCO_5             |         |           |5             |          |         |           |         |3.30   |          |           |                |
|P74       |ram_address<19>|IOB      |IO_L31N_5/D4       |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P75       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P76       |ram_address<18>|IOB      |IO_L32P_5/GCLK2    |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P77       |ram_address<17>|IOB      |IO_L32N_5/GCLK3    |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P78       |ram_address<16>|IOB      |IO/VREF_5          |OUTPUT   |LVCMOS33   |5             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P79       |ram_address<15>|IOB      |IO_L32P_4/GCLK0    |OUTPUT   |LVCMOS33   |4             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P80       |mclk           |IOB      |IO_L32N_4/GCLK1    |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P81       |               |DIFFM    |IO_L31P_4/DOUT/BUSY|UNUSED   |           |4             |          |         |           |         |       |          |           |                |
|P82       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P83       |init_b         |IOB      |IO_L31N_4/INIT_B   |OUTPUT   |LVCMOS33   |4             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P84       |               |         |VCCO_4             |         |           |4             |          |         |           |         |3.30   |          |           |                |
|P85       |sdi            |IOB      |IO/VREF_4          |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P86       |_scs<1>        |IOB      |IO_L30P_4/D3       |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P87       |_scs<2>        |IOB      |IO_L30N_4/D2       |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P88       |               |         |VCCINT             |         |           |              |          |         |           |         |1.2    |          |           |                |
|P89       |               |         |VCCAUX             |         |           |              |          |         |           |         |2.5    |          |           |                |
|P90       |sck            |IOB      |IO_L27P_4/D1       |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P91       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P92       |               |DIFFS    |IO_L27N_4/DIN/D0   |UNUSED   |           |4             |          |         |           |         |       |          |           |                |
|P93       |_scs<0>        |IOB      |IO                 |INPUT    |LVCMOS33   |4             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P94       |pwrled         |IOB      |IO_L25P_4          |OUTPUT   |LVCMOS33   |4             |12        |SLOW     |PULLUP     |         |       |LOCATED   |NO         |NONE            |
|P95       |_cpu_reset     |IOB      |IO_L25N_4          |OUTPUT   |LVCMOS33   |4             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P96       |_cpu_ipl<0>    |IOB      |IO/VREF_4          |OUTPUT   |LVCMOS33   |4             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P97       |_cpu_ipl<1>    |IOB      |IO                 |OUTPUT   |LVCMOS33   |4             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P98       |               |         |VCCO_4             |         |           |4             |          |         |           |         |3.30   |          |           |                |
|P99       |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P100      |_cpu_ipl<2>    |IOB      |IO_L01P_4/VRN_4    |OUTPUT   |LVCMOS33   |4             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P101      |cpu_clk        |IOB      |IO_L01N_4/VRP_4    |OUTPUT   |LVCMOS33   |4             |24        |FAST     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P102      |_cpu_dtack     |IOB      |IO/VREF_4          |OUTPUT   |LVCMOS33   |4             |12        |FAST     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P103      |               |         |DONE               |         |           |              |          |         |           |         |       |          |           |                |
|P104      |               |         |CCLK               |         |           |              |          |         |           |         |       |          |           |                |
|P105      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P106      |cpu_r_w        |IOB      |IO_L01P_3/VRN_3    |INPUT    |LVCMOS33   |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P107      |_cpu_lds       |IOB      |IO_L01N_3/VRP_3    |INPUT    |LVCMOS33   |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P108      |_cpu_uds       |IOB      |IO_L17P_3/VREF_3   |INPUT    |LVCMOS33   |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P109      |_cpu_as        |IOB      |IO_L17N_3          |INPUT    |LVCMOS33   |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P110      |               |         |VCCO_3             |         |           |3             |          |         |           |         |3.30   |          |           |                |
|P111      |cpu_data<0>    |IOB      |IO_L19P_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P112      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P113      |cpu_data<1>    |IOB      |IO_L19N_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P114      |cpu_data<2>    |IOB      |IO_L20P_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P115      |cpu_data<3>    |IOB      |IO_L20N_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P116      |cpu_data<4>    |IOB      |IO_L21P_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P117      |cpu_data<5>    |IOB      |IO_L21N_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P118      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P119      |cpu_data<6>    |IOB      |IO_L22P_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P120      |cpu_data<7>    |IOB      |IO_L22N_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P121      |               |         |VCCAUX             |         |           |              |          |         |           |         |2.5    |          |           |                |
|P122      |cpu_data<8>    |IOB      |IO_L23P_3/VREF_3   |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P123      |cpu_data<9>    |IOB      |IO_L23N_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P124      |cpu_data<10>   |IOB      |IO_L24P_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P125      |cpu_data<11>   |IOB      |IO_L24N_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P126      |cpu_data<12>   |IOB      |IO_L39P_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P127      |               |         |VCCO_3             |         |           |3             |          |         |           |         |3.30   |          |           |                |
|P128      |cpu_data<13>   |IOB      |IO_L39N_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P129      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P130      |cpu_data<14>   |IOB      |IO_L40P_3          |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P131      |cpu_data<15>   |IOB      |IO_L40N_3/VREF_3   |BIDIR    |LVCMOS33   |3             |4         |SLOW     |KEEPER     |NONE     |       |LOCATED   |NO         |NONE            |
|P132      |cpu_address<23>|IOB      |IO_L40P_2/VREF_2   |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P133      |cpu_address<22>|IOB      |IO_L40N_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P134      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P135      |cpu_address<21>|IOB      |IO_L39P_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P136      |               |         |VCCO_2             |         |           |2             |          |         |           |         |3.30   |          |           |                |
|P137      |cpu_address<20>|IOB      |IO_L39N_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P138      |cpu_address<19>|IOB      |IO_L24P_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P139      |cpu_address<18>|IOB      |IO_L24N_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P140      |cpu_address<17>|IOB      |IO_L23P_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P141      |cpu_address<16>|IOB      |IO_L23N_2/VREF_2   |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P142      |               |         |VCCAUX             |         |           |              |          |         |           |         |2.5    |          |           |                |
|P143      |cpu_address<15>|IOB      |IO_L22P_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P144      |cpu_address<14>|IOB      |IO_L22N_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P145      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P146      |cpu_address<13>|IOB      |IO_L21P_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P147      |cpu_address<12>|IOB      |IO_L21N_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P148      |cpu_address<11>|IOB      |IO_L20P_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P149      |cpu_address<10>|IOB      |IO_L20N_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P150      |cpu_address<9> |IOB      |IO_L19P_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P151      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P152      |cpu_address<8> |IOB      |IO_L19N_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P153      |               |         |VCCO_2             |         |           |2             |          |         |           |         |3.30   |          |           |                |
|P154      |cpu_address<7> |IOB      |IO/VREF_2          |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P155      |cpu_address<6> |IOB      |IO_L01P_2/VRN_2    |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P156      |cpu_address<5> |IOB      |IO_L01N_2/VRP_2    |INPUT    |LVCMOS33   |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P157      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P158      |               |         |TDO                |         |           |              |          |         |           |         |       |          |           |                |
|P159      |               |         |TCK                |         |           |              |          |         |           |         |       |          |           |                |
|P160      |               |         |TMS                |         |           |              |          |         |           |         |       |          |           |                |
|P161      |cpu_address<4> |IOB      |IO_L01P_1/VRN_1    |INPUT    |LVCMOS33   |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P162      |cpu_address<3> |IOB      |IO_L01N_1/VRP_1    |INPUT    |LVCMOS33   |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P163      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P164      |               |         |VCCO_1             |         |           |1             |          |         |           |         |3.30   |          |           |                |
|P165      |cpu_address<2> |IOB      |IO_L10P_1          |INPUT    |LVCMOS33   |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P166      |cpu_address<1> |IOB      |IO_L10N_1/VREF_1   |INPUT    |LVCMOS33   |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P167      |_joy1<3>       |IOB      |IO                 |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P168      |_joy1<4>       |IOB      |IO_L27P_1          |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P169      |_joy1<2>       |IOB      |IO_L27N_1          |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P170      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P171      |_joy1<1>       |IOB      |IO_L28P_1          |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P172      |_joy1<0>       |IOB      |IO_L28N_1          |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P173      |               |         |VCCAUX             |         |           |              |          |         |           |         |2.5    |          |           |                |
|P174      |               |         |VCCINT             |         |           |              |          |         |           |         |1.2    |          |           |                |
|P175      |_joy1<5>       |IOB      |IO                 |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P176      |_joy2<3>       |IOB      |IO_L31P_1          |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P177      |               |         |VCCO_1             |         |           |1             |          |         |           |         |3.30   |          |           |                |
|P178      |_joy2<4>       |IOB      |IO_L31N_1/VREF_1   |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P179      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P180      |_joy2<2>       |IOB      |IO_L32P_1/GCLK4    |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P181      |_joy2<1>       |IOB      |IO_L32N_1/GCLK5    |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P182      |_joy2<0>       |IOB      |IO                 |INPUT    |LVCMOS33   |1             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P183      |_joy2<5>       |IOB      |IO_L32P_0/GCLK6    |INPUT    |LVCMOS33   |0             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P184      |txd            |IOB      |IO_L32N_0/GCLK7    |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P185      |rxd            |IOB      |IO_L31P_0/VREF_0   |INPUT    |LVCMOS33   |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P186      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P187      |rts            |IOB      |IO_L31N_0          |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P188      |               |         |VCCO_0             |         |           |0             |          |         |           |         |3.30   |          |           |                |
|P189      |cts            |IOB      |IO                 |INPUT    |LVCMOS33   |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P190      |right          |IOB      |IO_L30P_0          |OUTPUT   |LVCMOS33   |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P191      |left           |IOB      |IO_L30N_0          |OUTPUT   |LVCMOS33   |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P192      |               |         |VCCINT             |         |           |              |          |         |           |         |1.2    |          |           |                |
|P193      |               |         |VCCAUX             |         |           |              |          |         |           |         |2.5    |          |           |                |
|P194      |_15khz         |IOB      |IO_L27P_0          |INPUT    |LVCMOS33   |0             |          |         |PULLUP     |NONE     |       |LOCATED   |NO         |NONE            |
|P195      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P196      |_hsync         |IOB      |IO_L27N_0          |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P197      |_vsync         |IOB      |IO                 |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P198      |blue<0>        |IOB      |IO_L25P_0          |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P199      |blue<1>        |IOB      |IO_L25N_0          |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P200      |blue<2>        |IOB      |IO/VREF_0          |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P201      |               |         |VCCO_0             |         |           |0             |          |         |           |         |3.30   |          |           |                |
|P202      |               |         |GND                |         |           |              |          |         |           |         |       |          |           |                |
|P203      |blue<3>        |IOB      |IO_L01P_0/VRN_0    |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P204      |green<0>       |IOB      |IO_L01N_0/VRP_0    |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P205      |green<1>       |IOB      |IO/VREF_0          |OUTPUT   |LVCMOS33   |0             |4         |SLOW     |NONE**     |         |       |LOCATED   |NO         |NONE            |
|P206      |               |         |HSWAP_EN           |         |           |              |          |         |           |         |       |          |           |                |
|P207      |               |         |PROG_B             |         |           |              |          |         |           |         |       |          |           |                |
|P208      |               |         |TDI                |         |           |              |          |         |           |         |       |          |           |                |
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen. 
****** Special VCCO requirements may apply. Please consult the device 
       family datasheet for specific guideline on VCCO requirements. 


